[bookmark: _Toc42488098]ANNEX II + III:	 TECHNICAL SPECIFICATIONS + TECHNICAL OFFER
[bookmark: _GoBack]Contract title: Supply contract for “Purchase of 10 drones for using in case of disasters/emergencies in the framework of SA RESILIENCE project, Programme IPA South Adriatic 2021-2027”
Publication reference: IPA-SA /RES-NCPA/SRV/13

Within the framework of the "SA Resilience" project, the IPA South Adriatic 2021-2027 Program, the National Civil Protection Agency is the Lead Partner.

The "SA Resilience" project has as its main objective to consolidate the mutual cooperation and coordination of the South Adriatic in the protection of civil protection, in order to undertake a strong protection, in order to undertake changes and others.

All this is intended to be achieved through increasing capacities in means and equipment, technological innovation, activities and human capacities.

Based on the Partnership Agreement, AKMC will purchase 10 Drones that will be used for emergency coordination and monitoring operations. 

Columns 1-2 should be completed by the contracting authority
Columns 3-4 should be completed by the tenderer
Column 5 is reserved for the evaluation committee 
Annex III - the contractor's technical offer
The tenderers are requested to complete the template on the next pages: 
· Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer), 
· Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)  
· Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation
The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.
The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

	1.
Item number/Quantity
	2.
Specifications required/Albanian for 10 drones (each drone should have all the parts specified below)
	3.
Specifications offered
	4. 
Notes, remarks, 
ref to documentation
	5.
Evaluation committee’s notes 

	10
	Albanian:
Pesha e Ngritjes:  5020±20 g
Shpejtësia maksimale e ngjitjes:  10 m/s
Shpejtësia maksimale e zbritjes:  8 m/s
Shpejtësia maksimale horizontale:  25 m/s
Lartësia maksimale e ngritjes:  7000 m
Koha maksimale e fluturimit: mbi 50 minuta
Shpejtësia Këndore Maksimale:  100°/s
Këndi Maksimal i Pjerrësisë:  35°
Temperatura e Funksionimit:  -20° deri në 50° C  Sistemi Satelitor Global i Navigimit (GNSS) :
GPS + Galileo + BeiDou + GLONASS*
IP 55 rezistent ndaj shiut

English:
Takeoff Weight: 5020±20 g
Maximum climb speed: 10 m/s
Maximum descent speed: 8 m/s
Maximum horizontal speed: 25 m/s
Maximum takeoff altitude: 7000 m
Maximum flight time: over 50 minutes Maximum angular velocity: 100°/s
Maximum pitch angle: 35°
Operating temperature: -20° to 50° C Global Navigation Satellite System (GNSS) :
GPS + Galileo + BeiDou + GLONASS*
IP 55 rain resistant

	
	
	

	10
	Albanian:
Diapazoni i Saktësisë së fluturimit (me erë  ose pa erë)
-Vertikal:
±0.1 m (me pozicionim vizual)
±0.5 m (me pozicionim satelitor)
±0.1 m (me pozicionim RTK)

-Horizontal:
±0.3 m (me pozicionim vizual)
±0.5 m (me pozicionim satelitor)
±0.1 m (me pozicionim RTK)

English
Flight Accuracy Range (with or without wind)
-Vertical:
±0.1 m (with visual positioning)
±0.5 m (with satellite positioning)
±0.1 m (with RTK positioning)

-Horizontal:
±0.3 m (with visual positioning)
±0.5 m (with satellite positioning)
±0.1 m (with RTK positioning)


	 
	
	

	10
	Albanian:
Saktësia RTK GNSS
Fiksimi RTK:
1 cm + 1 ppm (horizontale), 1.5 cm + 1 ppm (vertikale)
Drejtimi RTK
• Mbështet drejtimin RTK me një saktësi më të mirë se 2°
Hyrja ADS-B Ajrore
• E pajisur me marrës standard ajror ADS-B In dhe antena të dyfishta, duke mbështetur pritjen deri në 20 km.

Hapësirë ​​ruajtëse e brendshme  N/A

Porta USB-C Debug × 1: USB 2.0

English
RTK GNSS Accuracy
RTK Fix:
1 cm + 1 ppm (horizontal), 1.5 cm + 1 ppm (vertical)
RTK Direction
• Supports RTK direction with an accuracy of better than 2°
Airborne ADS-B In
• Equipped with standard airborne ADS-B In receiver and dual antennas, supporting reception up to 20 km.

Internal Storage N/A

USB-C Debug Port × 1: USB 2.0

	 
	
	

	10
	Albanian:
Gimbal
Ngarkesa Maksimale për Lidhësin e Vetëm të Gimbalit Sistemi Satelitor Global i Navigimit GNSS: 1400 g

English
Gimbal
Maximum Load for Single Gimbal Connector GNSS Global Navigation Satellite System: 1400 g
	
	
	

	10
	Albanian:
Ndjeshmëria
Lloji i Ndjeshmërisë: Sistem shikimi binokular omnidireksional (pamje rrethuese e ofruar nga sensorë shikimi me ngjyra të plota)

Mjedisi i Operacionit: Përpara, Prapa, Majtas, Djathtas dhe Lart

English:
Sensitivity
Sensitivity Type: Omnidirectional binocular vision system (surround view provided by full-color vision sensors)

Operation Environment: Front, Back, Left, Right and Up
	
	
	

	10
	Albanian:
Kamer termike H30 T dhe ndricim S1


English:
Thermal camera H30 T and lighting S1
	
	
	

	10
	
Albanian:
Kamera FPV
 Rezolucioni: • 1080p
 Fusha e Shikimit (FOV) : • DFOV: 150°
HFOV: 139.6°
VFOV: 95.3°

Shpejtësia e Kuadrove:   30fps
Distanca Maksimale e Transmetimit: 
- 40 km (FCC)
- 20 km (CE/SRRC/MIC)

English:
FPV Camera
Resolution: • 1080p
Field of View (FOV) : • DFOV: 150°
HFOV: 139.6°
VFOV: 95.3°

Frame Rate: 30fps
Maximum Transmission Distance:
- 40 km (FCC)
- 20 km (CE/SRRC/MIC)
	
	
	

	10
	Albanian:
Distanca Maksimale e Transmetimit (me ndërhyrje)
Ndërhyrje e fortë (ndërtesa të dendura, zona banimi, etj.): afërsisht 1.5-6 km
Ndërhyrje mesatare (qarqe periferike, parqe qyteti, etj.): afërsisht 6-15 km
Ndërhyrje e dobët (hapësira të hapura, zona të largëta, etj.): afërsisht 15-40 km

English:
Maximum Transmission Distance (with interference)
Strong interference (dense buildings, residential areas, etc.): approximately 1.5-6 km
Medium interference (suburban areas, city parks, etc.): approximately 6-15 km
Weak interference (open spaces, remote areas, etc.): approximately 15-40 km
	
	
	

	10
	Albanian:
Antenë
Antenë WLAN × 8: 6 antena të polarizuara vertikalisht dhe 2 antena të polarizuara horizontalisht
Mënyra e Funksionimit: 2T4R
English:
Antenna
WLAN Antenna × 8: 6 vertically polarized antennas and 2 horizontally polarized antennas
Operating Mode: 2T4R
	
	
	

	10
	Albanian:
Bateria (10 copë)
Kapaciteti:   20254 mAh
Numri i Cikleve:  minimumi 400
Protokolli Wi-Fi:   Wi-Fi Direct
Fuqia e Transmetuesit Bluetooth (EIRP) : < 10 dBm
Tb100 intelligjent+bateri station 
Kapaciteti i Ruajtjes:   RAM 8G + ROM 128G UFS + hapësirë ​​ruajtjeje e zgjerueshme nëpërmjet kartës microSD

English:
Battery (10 pieces)
Capacity: 20254 mAh
Number of Cycles: minimum 400
Wi-Fi Protocol: Wi-Fi Direct
Bluetooth Transmitter Power (EIRP): < 10 dBm
Tb100 intelligjent+bateri station
Storage Capacity: 8G RAM + 128G UFS ROM + expandable storage via microSD card
	
	
	

	10
	Albanian:
Spare parts: 
· 10 Hub 3.0 USB plus micro sd card reader (Për transferim të dhënash)
· 10 SD card min 256 gb

English:
Spare parts:
• 10 Hub 3.0 USB plus micro sd card reader (For data transfer)
• 10 SD cards min 256 gb
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